**Fig 1:** *J* – *V* characteristics of BHJ P3HT: PCBM – based devices of as cast and after thermal annealing from 50 - 175°C (in steps of 25°C, 10 min)