**Fig. 5:** A plot of carrier lifetimes as a function of thermal annealing temperatures.

As cast