**Fig. 6:** Mott-Schottky curve of ITO/PEDOT: PSS/P3HT: PCBM/Al device; as cast and after thermal annealing at 150°C.